Construction of Hollow Block Wall

Item	Description	Amount
A	Construction of Hollow Concrete Block Wall 190mm thick 21.00m (L) X 1.00m (H)	S$11,920.00
	i) Construction of Hollow Concrete Block Wall using labour, material, tools etc complete
	ii) Wall Plaster on both side with Skim coat - 42 m2
	iii) Painting for exterior Sealer & weatherproof paint
	Construction of Column Post (300mm x 300mm) with Plinth beam Using T13 & T16 Rebar - 21.00M Length
	i) RC Column - 14 nos with Footing including Labour, Material & Tools for excavation of depth of footing, rebar, and concrete.
B	Construction of Base Slab Using A7 BRC Mesh with 150mm thick with 500mm different level.	S$30,680.00
	i) Excavate and Levelling the ground and disposal of Soil
	ii) Base Slab for 500mm diff level using A7 BRC Mesh with 150mm thick Concrete including formwork etc. Completed
	iii) Back filling Soil and Top Portion Stone Chips between Wall & Rock Portion
	iv) RC Column & Base for Rock and Wall in between portion
	v) Floor Screeding with Design Tile for Open Auditorium including using labour, materials, tools, etc. complete – 100sft (Front Portion Only) (Sitting Area No Tiles)
	Construction of Column Post (300mm x 300mm) with Plinth beam Using T13 & T16 Rebar - 9.00m Length
	i) RC Column - 6 nos with Footing including Labour, Material & Tools for excavation of depth of footing, rebar, and concrete
	Construction of Hollow Concrete Block Wall 190mm thick 9.00m (L) X 1.00m (H)
	i) Construction of Hollow Concrete Block Wall using labour, material, tools etc complete
	ii) Wall Plaster on both side with Skim coat - 18 m2
	iii) Painting for exterior Sealer & weatherproof paint
	Fabrication & Installation of Steel Shelters with PVC Color roof sheet including column and bracing support
	Fabrication and installation for steel shelters using 50mm x 50mm SHS or 75mm x 75mm SHS with L angle frame bracing support
C	Construction and Installation of shelter for the walkway	S$17,000.00
	Installation of shelter for the walkway from behind the canteen up to the stairs connecting to the hall
	Installation of acrylic panel behind the exhaust pipe to block the air from blowing through the shelter
D	After the project completion: Cleaning of service work area Clearance of debris from the site Clearance of the bush surrounding the rock	S$600.00