Specification

1. Purchase Quantity: 24 Electronic Boards(Include Installation Supplementary Material), 13 Display(Include Installation Supplementary Material), 37 Desktop Computers, 37 Monitors, 12 Visualizer

2. Requirements

- Electronic Board

Details	Specifications
Touch Mode	IR Touch Sensor Mode
Surface	Anti-reflective Tempered Glass
Touch Tool	Hand or all objects
Touch Response Time	10ms or less
Display Type	UHD 55inch and above LED, UHD
Contrast Ratio	3000 : 1 or more
Brightness	300(cd/m2) or more
Maximum Resolution	3840 x 2160 (UHD) or more
Viewing Angle (Horizontal/Vertical)	Viewing Angle free (178°/178°, Min)
Output (RMS)	10W x 2 channels, stereo
Screen / Touch Mirroring	1:1 Bi-directional remote touch / mirroring capability required with Tablet PC Two-way class with smart pad without PC

- Display

Details	Specifications
Surface	Anti-reflection
Touch response time	10ms or less
Display type	UHD 66inch and above UHD
Contrast Ratio	3000 : 1 or more
Brightness	300(cd/m2) or more
Maximum Resolution	3840 x 2160 (UHD) or more
Viewing Angle (Horizontal/Vertical)	Viewing Angle free (178°/178°, Min)
Output (RMS)	10W X 2채널, 스테레오
Life span	50,000hrs
Dust protection function	IP5x(Dustproof coating)

- Desktop Computer (Main)

Details	Specifications
CPU	Intel CORE i5-6500 (3.2Ghz) (with noiseless cooler) or higher
Operating System	English Windows 10 or later
RAM	8GB
Hard Disk	HDD 1TB or more + SSD 256GB or more
Graphics	Intel HD Graphics 530 or higher Support DUAL monitor (D-SUB + DVI + HDMI) port method
LAN	10/100/1000Mbps or higher
Multi-memory card reader	Existing
Working Voltage	Free Voltage
컴퓨터형식 Computer Type	Tower type
Motherboard	H110 or higher
ODD	DVD-Multi 이상 DVD-Multi or higher
Manual	Provided (English manual)
Input Device	Keyboard: English keyboard Mouse: USB wheel mouse (2 buttons)
Restoration CD	Restore CD (restore CD to specification) and built-in restore image included

- Monitor

Details	Specifications
Screen size	LED 24 inches or more
Resolution (Aspect ratio)	1920×1080(16:9)
Function	Pivot function, Elevation function
Input terminals	D-SUB + DVI + HDMI
Brightness (cd / m2)	250 and above
Response rate	5m/s or less

- Visualizer

Details	Specifications
Image quality	4.0M pixels or more
Resolution	1920×1080(16:9)
Light source	LED
Digital Zoom	x10
image sensor	1/4″CMOS
Focus	Auto Focus
Frame	25fps
Scan area	최대 A3 Maximum A3
Connection	USB / VGA / HDMI

3. Others 기타사항

A. Singapore Korea International School may adjust options other than the above specifications for the goods delivered, in which case the prices may be adjusted in consultation with the manufacturer.

B. Other unspecified specifications and incidental equipment are the same as those for ordinary vehicles.

Other unspecified specifications and incidental materials shall be as provided by the school.